Ｍy　Ｑuestion

I will try to turn off SICMOS slowly when DESAT is activated.

How should I control Vgs during DESAT detection?

Please tell me how to select RSSD.

How do I set the DESAT voltage (DSH/L) detection level?



